> Performance Management
> This section contains additions and changes made to the performance commands available in this release. Topics covered in this chapter are:

> l | New Commands

> l | Modified Commands

> l | Obsoleted Commands

> l | GTPP Storage Server Changes

> l | Web Element Manager Changes

> New Commands
> This section contains performance management commands that are new in Release 9.0. New commands in this version are divided into the following sections:

> l | Common Commands - New in Release 9.0

> l | Content Filtering Commands - New in Release 9.0

> l | ECS Commands - New in Release 9.0

> l | Firewall Commands - New in Release 9.0

> l | GGSN Commands - New in Release 9.0

> l | HA Commands - New in Release 9.0

> l | NAT Commands - New in Release 9.0

> l | PDIF Commands - New in Release 9.0

> l | PDSN Commands - New in Release 9.0

> l | Peer-to-Peer - New in Release 9.0

> l | SGSN Commands - New in Release 9.0

> Common Commands - New in Release 9.0
> The following common commands are new in Release 9.0.
> None for this release.
> Content Filtering Commands - New in Release 9.0
> The following Content Filtering commands are new in Release 9.0.
> None for this release.
> ECS Commands - New in Release 9.0
> The following ECS commands are new in Release 9.0.
> None for this release.
> Firewall Commands - New in Release 9.0
> The following Stateful Firewall commands are new in Release 9.0.
> None for this release.
> GGSN Commands - New in Release 9.0
> The following GGSN commands are new in Release 9.0.
> show apn counter ip-allocation
> New command added to display IP allocation method information/statistics counters on per apn basis for all currently active calls.
> CLI (Exec Mode)
> show apn counter ip-allocation [all | name apn_name] [|{grep grep_options | more}]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show ip interface
> New keyword gre-keepalive added to this command to display states and statistics of GRE keepalive requests for GRE tunnel interface type IP interfaces.
> CLI (Exec Mode)
> show ip interface [vrf vrf-name] [ name intfc_name [statistics] [tunnel [gre-keepalive ] ] [summary] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> HA Commands - New in Release 9.0
> The following HA commands are new in Release 9.0.
> None for this release.
> NAT Commands - New in Release 9.0
> The following NAT commands are new in Release 9.0.
> None for this release.
> PDIF Commands - New in Release 9.0
> The following PDIF commands are new in Release 9.0.
> None for this release.
> PDSN Commands - New in Release 9.0
> The following PDSN commands are new in Release 9.0.
> None for this release.
> Peer-to-Peer - New in Release 9.0
> The following P2P commands are new in Release 9.0.
> show active-charging p2p-dynamic-rules
> This command displays P2P Dynamic signature file information.
> CLI (Exec Mode)
> show active-charging p2p-dynamic-rules [ verbose ] [ acsmgr instance instance_id ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> SGSN Commands - New in Release 9.0
> The following SGSN commands are new in Release 9.0.
> None for this release.
> Modified Commands
> This section contains performance management commands that have been modified in Release 9.0. Modified commands in this version are divided into the following sections:

> l | Common Commands - Modified in Release 9.0

> l | Content Filtering Commands - Modified in Release 9.0

> l | ECS Commands - Modified in Release 9.0

> l | Firewall Commands - Modified in Release 9.0

> l | GGSN Commands - Modified in Release 9.0

> l | HA Commands - Modified in Release 9.0

> l | NAT Commands - Modified in Release 9.0

> l | PDIF Commands - Modified in Release 9.0

> l | PDSN Commands - Modified in Release 9.0

> l | Peer-to-Peer Commands - Modified in Release 9.0

> l | Session Control Manager Commands - Modified in Release 9.0

> l | SGSN Commands - Modified in Release 9.0

> Common Commands - Modified in Release 9.0
> The following common commands have been modified in Release 9.0.
> clear active-charging credit-control statistics
> This command clears Credit Control statistics. The server keyword and options were added to this command. This enables clearing per Diameter server statistics of Gy messages.
> CLI (Exec Configuration Mode)
> clear active-charging credit-control statistics [ group group_name ] [ server { ip-address ip_address [ port port_number ] | name server_name } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear crypto
> New ipsec-3gpp-cscf keyword added.
> CLI (Exec Configuration Mode)
> clear crypto { isakmp [ tag map_name | peer peer_ip ] | security-association { counters tag map_name [ tx | rx ] | tag map_name | peer peer_ip } | statistics { ikev2 | ipsec-3gpp-cscf } [service-ip-address ip-address | service-name name ] }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> clear ims-authorization policy-control
> This command clears statistics for all or for a specified IMS Authorization Service or server. The server keyword and options were added to this command, which enables to select a specific server.
> CLI (Exec Configuration Mode)
> clear ims-authorization { policy-control statistics [ service ims_auth_svc_name | server { ip-address ip_address [ port port_value ] | name server_name } ] | service statistics [ name service_name ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> monitor protocol
> Activates monitor function to examine protocol-specific information based on protocol. The following protocol was added to the list of protocols:

> l | ICAP

> CLI (Exec Mode)
> monitor protocol
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> monitor subscriber username
> Activates monitor function to examine protocol-specific information based on subscriber within current context. The following protocol was added to the list of protocols:

> l | ICAP

> CLI (Exec Mode)
> monitor subscriber username user_name
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging credit-control
> This command displays Credit Control statistics. The server keyword and options were added to this command. This enables to view per Diameter server statistics of Gy messages.
> CLI (Exec Configuration Mode)
> show active-charging credit-control { { statistics [ group group_name ] [ server { ip-address ip_address [ port port_number ] | name server_name } ] } | { session-states [ rulebase rulebase_name ] [ content-id content_id ] } } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging fw-and-nat policy name
> This command displays the Firewall-and-NAT Policy information. The output of this command now includes the following new fields with NAT related configurations and Firewall feature level configurations added:

> l | Action upon receiving TCP SYN packet with ECN/CWR Flag set

> l | Action upon receiving a malformed packet

> l | Action upon IP Reassembly Failure

> l | Action upon receiving an IP packet with invalid Options

> l | Action upon receiving a TCP packet with invalid Options

> l | Action upon receiving an ICMP packet with invalid Checksum

> l | Action upon receiving a TCP packet with invalid Checksum

> l | Action upon receiving an UDP packet with invalid Checksum

> l | TCP Stateful Checks

> l | First Packet Non-SYN Action

> l | ICMP Stateful Checks

> l | NAT Configuration

> l | NBR Format

> l | Private IP NPU Flow Timeout

> l | Suppress sending NAT bind update to AAA

> CLI (Exec Mode)
> show active-charging fw-and-nat policy { { { all | name fw_nat_policy } [ service name acs_service ] } | { statistics { all | name fw_nat_policy } } } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show ims-authorization policy-control
> This command displays information and statistics specific to policy control in IP Multimedia Subsystem (IMS) authorization service. The server keyword and options were added to this command, which enables to select a specific server.
> CLI (Exec Mode)
> show ims-authorization policy-control statistics [ service ims_auth_svc_name | server { ip-address ip_address [ port port_value ] | name server_name } ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show rohc
> Modified command to add summary output and support HSGW-RoHC.
> CLI (Exec Mode)
> show rohc { counters [ all | callid call_id | msid msid_num |
> imsi imsi_num | username user_name ] | statistics | summary [ all | callid call_id | msid msid_num | imsi imsi_num | username user_name ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Content Filtering Commands - Modified in Release 9.0
> The following Content Filtering commands have been modified in Release 9.0.
> clear content-filtering category statistics
> This command clears all Category-based Content Filtering application statistics, or statistics for a specific SRDB Manager instance. This release onwards the SRDB Manager instance number can be specified as any integer from 1 through 10000.
> CLI (Exec Mode)
> clear content-filtering category statistics [ facility srdbmgr instance instance_value ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging content-filtering category statistics
> This command displays category-based content filtering statistics for rulebase(s). The following Dynamic Content Filtering feature related fields were added to the output of this command:

> l | Cumulative Dynamic Content Filtering Statistics

> l | Dynamic Flows discarded

> l | Dynamic Flows redirected

> l | Dynamic Flows allowed

> l | Dynamic Flows terminated

> l | Dynamic Flows discarded with content insertion

> l | Total Dynamic Flows blocked

> l | Total Number of dynamic lookups

> l | Total number of unknown URLs

> l | Dynamic Failure Action (Rating Attempts Not Completed):

> l | Flows discarded

> l | Flows redirected

> l | Flows allowed

> l | Flows terminated

> l | Flows discarded with content insertion

> l | Total Flows blocked

> l | Time taken for Dynamic rating

> l | Number of URLs

> l | Attempts not completed

> CLI (Exec Mode)
> show active-charging content-filtering category statistics [ rulebase { name rulebase_name | all } ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging content-filtering server-group statistics
> This command displays information for Content Filtering Server Group(s) configured in the service. The following changes were made to this command:

> l | The verbose option was added. This enables viewing ICAP queue length statistics.

> l | The output of this command now displays the histogram of ICAP server's response time.

> CLI (Exec Mode)
> show active-charging content-filtering server-group [ statistics [ verbose ] ] [ name cfsg_name ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show content-filtering category database facility srdbmgr
> This command displays details of the specified category-based content filtering database for content filtering application configured in a system/service. The following Dynamic Content Filtering feature related fields were added to the output of this command:

> l | Dynamic SRDB Instance

> l | RaterPkg Load Status

> l | Number of Model files

> l | Standby Dynamic SRDB Instance

> l | RaterPkg Load Status

> l | Number of Model files

> CLI (Exec Mode)
> show content-filtering category database facility srdbmgr { all | instance instance_value } [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show content-filtering category statistics facility srdbmgr
> This command displays statistics for the Category-based Content Filtering application configured in a system/service. The following Dynamic Content Filtering feature related fields were added to the output of this command:

> l | Dynamic Content Filtering SRDB Instance Based Statistics:

> l | Instance Number

> l | Dynamic Rating:

> l | Request Count

> l | Response Total

> l | Response Successful

> l | Response Not Rated

> CLI (Exec Mode)
> show content-filtering category statistics facility srdbmgr { all | instance instance_value } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show content-filtering category url <url> policy-id <id> verbose
> This command displays the category-based content filtering statistics at the specific URL configured in a system/service. The output of this command now includes the following new fields with Dynamic CF enabled/disabled:

> l | Action Configured

> l | Content Insertion String

> l | Redirect URL

> CLI (Exec Mode)
> show content-filtering category url url_string
> [ policy-id cf_policy_id | rulebase rulebase_name ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging content-filtering category statistics
> This command displays the category-based content filtering statistics. The output of this command now includes the following new field for dynamic rating only if the response code is in the range 2xx:

> l | Response codes not in range 2xx

> CLI (Exec Mode)
> show active-charging content-filtering category statistics [ rulebase { name rulebase_name | all } ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show content-filtering category statistics facility srdbmgr all
> This command displays the statistics for category-based content filtering application configured in a system/service. The output of this command now includes the following new Dynamic Content Filtering feature related field:

> l | Histogram for number of URLs hit per SN category (sorted on no. of URLs)

> CLI (Exec Mode)
> show content-filtering category statistics [ facility srdbmgr { all | instance instance_value }] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging content-filtering category statistics
> This command displays the category-based content filtering statistics. The output of this command now includes the following new fields:

> l | Number of Packets Hit per Category

> l | Number of Packets Blocked per Category

> CLI (Exec Mode)
> show active-charging content-filtering category statistics [ rulebase { name rulebase_name | all } ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> ECS Commands - Modified in Release 9.0
> The following ECS commands have been modified in Release 9.0.
> show active-charging service
> This command displays Active Charging Service details. The output of this command includes the following new field:

> l | Dynamic Content Filtering: Indicates whether Dynamic Content Filtering is enabled or disabled.

> CLI (Exec Mode)
> show active-charging service { all | name svc_name } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging analyzer statistics
> This command displays statistic information for protocol analyzers. The following fields were added to this command’s output:

> l | IPv6

> l | ICMPv6

> l | ACS IPv6 Session Stats:

> l | Total Uplink Bytes

> l | Total Downlink Bytes

> l | Total Uplink Pkts

> l | Total Downlink Pkts

> l | Uplink Bytes Fragmented

> l | Downlink Bytes Fragmented

> l | Uplink Pkts Fragmented

> l | Downlink Pkts Fragmented

> l | Uplink Bytes Invalid

> l | Downlink Bytes Invalid

> l | Uplink Pkts Invalid

> l | Downlink Pkts Invalid

> l | ACS ICMPv6 Session Stats:

> l | Total Uplink Bytes

> l | Total Downlink Bytes

> l | Total Uplink Pkts

> l | Total Downlink Pkts

> l | ECHO Request

> l | ECHO Reply

> l | Dst Unreachable

> l | Parameter Problem

> l | Time Exceeded

> l | Packet Too Big

> l | Other ICMP Req

> l | Invalid Pkts

> CLI (Exec Mode)
> show active-charging analyzer statistics { name protocol [ verbose ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging analyzer statistics name
> This command displays Active Charging protocol analyzer statistics for the specified analyzer. The ipv6 and icmpv6 keywords were added to this command.
> CLI (Exec Mode)
> show active-charging analyzer statistics name { dns | file-transfer | ftp | http | icmp | icmpv6 | imap | ip | ipv6 | mms | p2p | pop3 | rtcp | rtp | rtsp | sdp | secure-http | sip | smtp | tcp | udp | wsp | wtp } [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging analyzer statistics name dns
> This command displays Active Charging protocol analyzer statistics for the DNS analyzer. With the support for IPv6 in ACS, AAAA record type is supported in DNS for IPv6 addresses. The output of this command now includes the following new fields corresponding to support AAAA record type in DNS for IPv6:

> l | Request:

> l | AAAA Query Type

> l | Response:

> l | AAAA Query Type

> CLI (Exec Mode)
> show active-charging analyzer statistics name dns [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging sessions full all
> This command displays statistics for Active Charging Service Sessions. The output of this command includes the following new fields:

> l | Client-IP

> l | Current IPv6 Flows

> l | Current ICMPv6 Flows

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] [ [ all ] | [ filters_keywords ] + ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging flows type
> This command displays information on flows filtered by flow type of application protocol. The ipv6 and icmpv6 options were added to this command.
> CLI (Exec Mode)
> show active-charging flows type { dns | ftp | http | icmp | icmpv6 | imap | ip | ipv6 | mms | p2p | pop3 | rtcp | rtp | rtsp | secure-http | sip | smtp | tcp | udp | unknown | wsp-connection-less | wsp-connection-oriented } [ options ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging flows ip-address
> This command displays active charging flows in a system or service. This command now accepts IPv6 addresses.
> CLI (Exec Mode)
> show active-charging flows { all | [ connected-time [ < | > | greater-than | less-than ] seconds ] [ flow-id flow_id ] [ full ] [ idle-time [ < | > | greater-than | less-than ] seconds ] [ ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address ] [ nat { not-required | required [ nat-ip nat_ip_address ] } ] [ port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number ] [ rx-bytes [ < | > | greater-than | less-than ] number ] [ rx-packets [ < | > | greater-than | less-than ] number ] [ session-id session_id ] [ summary ] [ trans-proto { icmp | tcp | udp } ] [ tx-bytes [ < | > | greater-than | less-than ] number ] [ tx-packets [ < | > | greater-than | less-than] number ] [ type flow_type ] } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging rulebase statistics
> This command displays statistical information for all/the specified rulebase. The output of this command now includes the following new field:

> l | EDRs generated for voip call end

> CLI (Exec Mode)
> show active-charging rulebase statistics [ name rulebase_name ] | [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Firewall Commands - Modified in Release 9.0
> The following Stateful Firewall commands have been modified in Release 9.0.
> show active-charging firewall statistics verbose
> This command displays the Active Charging Stateful Firewall statistics. The output of this command now includes the following new field to control the behavior of Firewall on receiving TCP SYN packets with either ECE/CWR Flags set:

> l | SYN Packets Dropped due to ECE/CWR Set

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | ip | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> GGSN Commands - Modified in Release 9.0
> The following GGSN commands have been modified in Release 9.0.
> show subscribers ggsn-only summary
> Following counters added to the output of this command to display the statistics for the overcharging protection support due to loss of radio coverage (LORC):

> l | out packet dropped due to lorc

> l | ggsn LORC state

> CLI (Exec Mode)
> show subscribers ggsn-only [summary]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show subscribers ggsn-only full
> Following counters added to the output of this command to display the statistics for the overcharging protection support due to loss of radio coverage (LORC):

> l | GGSN LORC State

> l | output pkts dropped due to lorc

> CLI (Exec Mode)
> show subscribers ggsn-only full
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpc full
> Following counter added to the output of this command to display the statistics for the overcharging protection support due to loss of radio coverage (LORC):

> l | Transitions to LORC state

> CLI (Exec Mode)
> show gtpc full
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpc statistics
> New keyword custom2 and following counters added to the output of this command with filter custom2 to display the statistics for the overcharging protection support due to loss of radio coverage (LORC):

> l | LORC Stats

> l | Sessions in lorc state

> l | Transitions to lorc state

> CLI (Exec Mode)
> show gtpc statistics [ apn-name apn_name ] [ custom1 | custom2] [sgsn-address address ] [ ggsn-service svc_name ] [ verbose ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> HA Commands - Modified in Release 9.0
> The following HA commands have been modified in Release 9.0.
> None for this release.
> NAT Commands - Modified in Release 9.0
> The following NAT commands have been modified in Release 9.0.
> None for this release.
> PDIF Commands - Modified in Release 9.0
> The following PDIF commands have been modified in Release 9.0.
> None for this release.
> PDSN Commands - Modified in Release 9.0
> The following PDSN commands have been modified in Release 9.0.
> None for this release.
> Peer-to-Peer Commands - Modified in Release 9.0
> The following Peer-to-Peer commands have been modified in Release 9.0.
> None for this release.
> show active-charging rulebase statistics name
> This command displays details of the active-charging rulebase statistics configured in a system/service. The output of this command now includes the following new fields to support Random Drop as a charging action to degrade voice quality:

> l | P2P random drop stats

> l | Total Dropped Packets

> l | Total Dropped Packet Bytes

> CLI (Exec Mode)
> show active-charging rulebase { { { all | name rulebase_name } [ service name acs_service ] } | statistics [ name rulebase_name ] } | [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging analyzer statistics name p2p verbose
> This command displays details of the active-charging statistics for protocol analyzers configured in a system/service. The output of this command now includes the following fields to support the new protocols:

> l | Freenet

> l | Aimini

> l | Battlefld

> l | Openft

> l | Qqgame

> l | Quake

> l | Secondlife

> l | Actsync

> l | Nimbuzz

> l | Iax

> l | Paltalk

> l | Warcft3

> l | Rdp

> l | Iptv

> l | Pandora

> CLI (Exec Mode)
> show active-charging analyzer statistics name p2p [ verbose ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging sessions summary
> This command displays the statistics for Active Charging service sessions. The output of this command now includes the following fields to support the new P2P protocols:

> l | Current FREENET Sessions

> l | Current AIMINI Sessions

> l | Current BATTLEFIELD Sessions

> l | Current OPENFT Sessions

> l | Current QQGAME Sessions

> l | Current QUAKE Sessions

> l | Current SECONDLIFE Sessions

> l | Current ACTIVESYNC Sessions

> l | Current NIMBUZZ Sessions

> l | Current IAX Sessions

> l | Current PALTALK Sessions

> l | Current WARCRAFT3 Sessions

> l | Current IPTV Sessions

> l | Current RDP Sessions

> l | Current PANDORA Sessions

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show active-charging sessions summary type p2p
> This command displays the statistics for specific Active Charging service sessions. The output of this command now includes the following fields to support the new P2P protocols:

> l | Current FREENET Sessions

> l | Current AIMINI Sessions

> l | Current BATTLEFIELD Sessions

> l | Current OPENFT Sessions

> l | Current QQGAME Sessions

> l | Current QUAKE Sessions

> l | Current SECONDLIFE Sessions

> l | Current ACTIVESYNC Sessions

> l | Current NIMBUZZ Sessions

> l | Current IAX Sessions

> l | Current PALTALK Sessions

> l | Current WARCRAFT3 Sessions

> l | Current IPTV Sessions

> l | Current RDP Sessions

> l | Current PANDORA Sessions

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Session Control Manager Commands - Modified in Release 9.0
> The following SCM commands have been modified in Release 9.0.
> None for this release.
> SGSN Commands - Modified in Release 9.0
> The following SGSN commands have been modified in Release 9.0.
> None for this release.
> Obsoleted Commands
> This section contains performance management commands that have been obsoleted in Release 9.0. Obsoleted commands in this version are divided into the following sections:

> l | Common Commands - Obsoleted from Release 9.0

> l | Content Filtering Commands - Obsoleted from Release 9.0

> l | ECS Commands - Obsoleted from Release 9.0

> l | Firewall Commands - Obsoleted from Release 9.0

> l | GGSN Commands - Obsoleted from Release 9.0

> l | HA Commands - Obsoleted from Release 9.0

> l | NAT Commands - Obsoleted from Release 9.0

> l | PDSN Commands - Obsoleted from Release 9.0

> l | Peer-to-Peer Commands - Obsoleted from Release 9.0

> l | SGSN Commands - Obsoleted from Release 9.0

> Common Commands - Obsoleted from Release 9.0
> The following common commands have been obsoleted in Release 9.0.
> show css delivery-sequence
> With the external CSS server feature no longer being supported, this command has been obsoleted.
> CLI (Exec Mode)
> show css delivery-sequence{ all | name seq_name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show css server
> With the external CSS server feature no longer being supported, this command has been obsoleted.
> CLI (Exec Mode)
> show css server { all | name server_name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show css service
> With the external CSS server feature no longer being supported, this command has been obsoleted.
> CLI (Exec Mode)
> show css service { all | name service_name }
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Content Filtering Commands - Obsoleted from Release 9.0
> The following Content Filtering commands have been obsoleted in Release 9.0.
> None for this release.
> ECS Commands - Obsoleted from Release 9.0
> The following ECS commands have been obsoleted in Release 9.0.
> None for this release.
> Firewall Commands - Obsoleted from Release 9.0
> The following Stateful Firewall commands have been obsoleted in Release 9.0.
> None for this release.
> GGSN Commands - Obsoleted from Release 9.0
> The following GGSN commands have been obsoleted in Release 9.0.
> None for this release.
> HA Commands - Obsoleted from Release 9.0
> The following HA commands have been obsoleted in Release 9.0.
> None for this release.
> NAT Commands - Obsoleted from Release 9.0
> The following NAT commands have been obsoleted in Release 9.0.
> None for this release.
> PDSN Commands - Obsoleted from Release 9.0
> The following PDSN commands have been obsoleted in Release 9.0.
> None for this release.
> Peer-to-Peer Commands - Obsoleted from Release 9.0
> The following Peer-to-Peer commands have been obsoleted in Release 9.0.
> None for this release.
> SGSN Commands - Obsoleted from Release 9.0
> The following SGSN commands have been obsoleted in Release 9.0.
> None for this release.
> GTPP Storage Server Changes
> The following commands have been modified in Release 9.0.
> show gtpp storage-server status
> This command displays details of the configured GTPP storage server. The following new fields have been added to the output of this command to support additional disks monitored by GSS, and to monitor the GSS Disk partition space:

> l | Resource Monitor:

> l | Available Disk Gss Datafile Path (GB)

> l | Available Disk Gss Install Path (GB)

> l | Available Disk Gss Database Path (GB)

> l | Resource Monitor Status:

> l | Available Disk Gss Datafile Path (GB)

> l | Available Disk Gss Install Path (GB)

> l | Available Disk Gss Database Path (GB)

> CLI (Exec Mode)
> show gtpp storage-server [ counters { all | group name name } | group name name | local file { counters { all | group name name } | statistics [ group name name ] } | status [ verbose ] | streaming { counters { all | group name name } | statistics [ group name name ] } ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpp storage-server streaming file statistics
> New counter Total Files Failed added to indicate the number of CDR files failed for streaming due to any reason to remote storage.
> CLI (Exec Mode)
> show gtpp storage-server [ counters { all | group name name } | group name name | local file { counters { all | group name name } | statistics [ group name name ] } | status [ verbose ] | streaming file { counters { all | group name name } | statistics [ group name name ] } ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> show gtpp storage-server streaming file statistics verbose
> New counter CDR distribution in DRT Messages added to indicate the distribution of CDRs in DRT messages.
> CLI (Exec Mode)
> show gtpp storage-server [ counters { all | group name name } | group name name | local file { counters { all | group name name } | statistics [ group name name ] } | status [ verbose ] | streaming file { counters { all | group name name } | statistics [ group name name ] } ] [ | { grep grep_options | more } ]
> Web Element Manager Path
> This functionality is not supported at this time on the Web Element Manager.
> Web Element Manager Changes
> There were no Web Element Manager changes in Release 9.0.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883