> GT-Format2 Configuration Mode Commands
> The GT-Format2 configuration mode is a sub-mode for either the Global Title Translation Association configuration mode or the Global Title Translation Address-Map configuration mode. This sub-mode configures a set of rules used in the global title translation (GTT) process.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the configuration mode and returns to the Global configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the Global configuration mode.
> translation-type
> Configures the translation type to be applied during the translation process.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> translation-type number
> number
> Must be an integer between 0 and 255.
> Default is 0
> Usage
> Use this command to configure the GTT translation type to be applied during global title translation process.
> Example
> translation-type 232

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883